

**SH Series Specifications**

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Capacity | Stroke | Travel/Rotation |
| SH-110 or SH-110-S | 110 lbf | - | - |
| SH-220 or SH-220-S | 220 lbf | 11.8" (300mm) | 1.2mm |
| SH-750 or SH-750-S | 750 lbf | 14.5" (370mm) | 0.6mm |

**Standard Distance Meter Specifications**

|  |  |
| --- | --- |
| Display | Push button for inch/mm, zero set and on/off |
| Resolution | 0.0005"/0.01 mm |
| Accuracy | 0.1% of reading or 0.005"/0.1 mm whichever is greater |